------------------------------------------------------------------------------
1.  CHEMICAL PRODUCT AND COMPANY IDENTIFICATION

Product Name: KODAK AQUA-IMAGE Cleaner/Preserver

Catalog Number(s):       833 3635 - 1 quart (U.S.)

Manufacturer/Supplier: EASTMAN KODAK COMPANY, Rochester, New York 14650

For Emergency Health, Safety & Environmental Information, call (585) 722-5151

For other information or to request an MSDS, call (800) 242-2424.

Synonym(s):   CIN 10068023; KAN 355388; PCD 3855/40420; E-0001.000; CAT#
              1312289

------------------------------------------------------------------------------
2.  COMPOSITION/INFORMATION ON INGREDIENTS

Weight % - Component - (CAS Registry No.)

 60-65     Stoddard Solvent (008052-41-3)
 20-30     Water (007732-18-5)
  5-10     Glycerol (000056-81-5)
   2       Phosphoric acid (007664-38-2)
  1-5      Sodium phosphate, dibasic (007558-79-4)
  1-5      Polyvinylpyrrolidone (009003-39-8)

------------------------------------------------------------------------------
3.  HAZARDS IDENTIFICATION

CONTAINS: Stoddard Solvent (008052-41-3); Phosphoric acid (007664-38-2)

WARNING!
COMBUSTIBLE LIQUID AND VAPOR
NOTICE! DELIBERATE CONCENTRATION AND INHALATION OF VAPORS MAY BE HARMFUL OR
FATAL
MAY BE HARMFUL IF SWALLOWED
CAUSES SKIN AND EYE IRRITATION
HIGH VAPOR CONCENTRATIONS MAY CAUSE DROWSINESS AND IRRITATION OF THE EYES OR
RESPIRATORY TRACT
CAN CAUSE CNS EFFECTS

Eastman Kodak Hazard Ratings: R-1, S-2, F-2, C-0

HMIS Hazard Ratings:
Health -  2, Flammability - 2, Reactivity - 0, Personal Protection - B

NFPA Hazard Ratings:
Health - 1, Flammability - 2, Reactivity (Stability) - 0

NOTE: HMIS and NFPA hazard indexes involve data review and interpretation that
may vary among companies. They are intended only for rapid, general
identification of the magnitude of the potential hazards. The personal
protection index is only intended for general guidance on personal protection
equipment (PPE) that is suitable for the potential hazards of the material.
PPE (e.g., respirators) may not be needed if engineering controls (e.g., local
ventilation) are adequate. An asterisk (*), in the HMIS health field,
designates potential chronic or target organ hazards. To adequately address
safe handling, ALL information in this MSDS must be considered.

------------------------------------------------------------------------------
4.  FIRST-AID MEASURES

Inhalation: If symptomatic, move to fresh air. Treat symptomatically. Get
medical attention if symptoms persist.

Eyes: Immediately flush with plenty of water for at least 15 minutes. Get
medical attention.

Skin: Immediately flush with plenty of water for at least 15 minutes while
removing contaminated clothing and shoes. Get medical attention if symptoms
occur. Wash contaminated clothing before reuse. Destroy or thoroughly clean
contaminated shoes.

Ingestion: Do NOT induce vomiting. Give victim a glass of water. Never give
anything by mouth to an unconscious person. Call a physician or poison control
center immediately.

------------------------------------------------------------------------------
5.  FIRE FIGHTING MEASURES

Extinguishing Media: Water spray, carbon dioxide (CO2), dry chemical, alcohol
foam

Special Fire-Fighting Procedures: Wear self-contained breathing apparatus and
protective clothing. Use water spray to keep fire-exposed containers cool.

Hazardous Combustion Products: Carbon dioxide, carbon monoxide

Unusual Fire and Explosion Hazards: Classified as combustible. Material
contains a combustible solvent that may accumulate in the container headspace.

------------------------------------------------------------------------------
6.  ACCIDENTAL RELEASE MEASURES

Eliminate all ignition sources. Absorb spill with vermiculite or other inert
material, then place in a container for chemical waste. Clean surface
thoroughly to remove residual contamination.
------------------------------------------------------------------------------
7.  HANDLING AND STORAGE

Personal Precautionary Measures: Avoid contact with eyes, skin, and clothing.
Avoid prolonged or repeated breathing of mist or vapor. Use with adequate
ventilation. Wash thoroughly after handling.

Prevention of Fire and Explosion: Keep from contact with oxidizing materials.
Keep away from heat and flame. Use with adequate ventilation.

Storage: Keep container closed.

------------------------------------------------------------------------------
8.  EXPOSURE CONTROLS/PERSONAL PROTECTION

Exposure Limits:

  ACGIH Threshold Limit Value (TLV):

    Phosphoric acid: 1 mg/m3 TWA; 3 mg/m3 STEL
    Stoddard Solvent: 100 ppm TWA
    Glycerol as glycerin mist: 10 mg/m3

  OSHA (USA) Permissible Exposure Limit (PEL - 1971 Table Z-1 Values):

    Phosphoric acid: 1 mg/m3 TWA
    Stoddard Solvent: 500 ppm TWA; 2900 mg/m3 TWA
    Glycerol as glycerin mist: 5 mg/m3 respirable fraction

Ventilation: Good general ventilation (typically 10 air changes per hour)
should be used. Ventilation rates should be matched to conditions.
Supplementary local exhaust ventilation, closed systems, or respiratory
protection may be needed in special circumstances such as poorly ventilated
spaces, evaporation from large surfaces, spraying, heating, etc.

Respiratory Protection: If engineering controls do not maintain airborne
concentrations below recommended exposure limits, an approved respirator must
be worn. Respirator type: Full-face with organic vapor/acid gas & P95
particulate filter. If respirators are used, a program should be instituted to
assure compliance with OSHA Standard 29 CFR 1910.134.

Eye Protection: Wear safety glasses with side shields (or goggles).

Skin Protection: Wear impervious gloves and protective clothing appropriate
for the risk of exposure.

Recommended Decontamination Facilities: Eye bath, washing facilities, safety
shower

------------------------------------------------------------------------------
9.  PHYSICAL AND CHEMICAL PROPERTIES

Physical Form: Liquid (emulsion)
Color: Milky white
Odor: Aromatic
Specific Gravity (water = 1): 0.89
Vapor Pressure at 20°C (68°F): 28 mbar (21 mm Hg)
Vapor Density (Air = 1): 0.8
Volatile Fraction by Weight: 85 %
Boiling Point: >100°C (>212°F)
Solubility in Water: Complete
pH: Not available
Flash Point: 47°C (116°F)  (estimated)

------------------------------------------------------------------------------
10. STABILITY AND REACTIVITY

Stability: Stable
  No exotherm to: boiling

Incompatibility: Strong oxidizing agents

Hazardous Polymerization: Will not occur.

------------------------------------------------------------------------------
11. TOXICOLOGICAL INFORMATION

Effects of Exposure:

  General:

    Contains Phosphoric acid. The following exposure effects are based on pH
    of the solution, concentration of the acid, and a review of the
    literature.

    Contains Stoddard Solvent. Can cause CNS effects.

  Inhalation: High vapor concentrations may cause drowsiness and irritation.
  Deliberate concentration and inhalation of vapors may be harmful or fatal.

  Eyes: Causes irritation. High vapor concentrations may cause irritation.

  Skin: Causes irritation.

  Ingestion: May be harmful if swallowed. May cause irritation of the
  gastrointestinal tract. If aspirated into lungs during swallowing or
  vomiting, it may cause pulmonary hemorrhage, edema and possible death.

------------------------------------------------------------------------------
12. ECOLOGICAL INFORMATION

The following properties are ESTIMATED from the components of the
preparations.
However, this material, itself, has not been tested for environmental effects.

 Potential Toxicity

       Fish LC50 mg/l:               10-100
    Daphnid EC50 mg/l:               10-100
       Algal IC50 mg/l:              1-10

 Organics Readily Degradable        Yes (7 days)
 (>70%):
 Potential Bioaccumulation:         Log Pow <1

 COD (approximate g/l):             104
 BOD5 (approximate g/l):            110

 Potential Toxicity
 Waste treatment microorganisms     Not available
 EC50 (mg/l):

------------------------------------------------------------------------------
13. DISPOSAL CONSIDERATIONS

Discharge, treatment, or disposal may be subject to national, state, or local
laws. Contract with a licensed chemical disposal agency. Since emptied
containers retain product residue, follow label warnings even after container
is emptied.

------------------------------------------------------------------------------
14. TRANSPORT INFORMATION

- For transportation information regarding this product call the Kodak
Worldwide Transportation Hazmat Hot Line: (585) 722-2400 between 8 a.m. and 5
p.m. (Eastern Standard Time), Monday through Friday.

------------------------------------------------------------------------------
15. REGULATORY INFORMATION

- Material(s) known to the State of California to cause cancer: None
- Material(s) known to the State of California to cause adverse reproductive
  effects: None

- Carcinogenicity Classification (components present at 0.1% or more):
  - International Agency for Research on Cancer (IARC): None
  - American Conference of Governmental Industrial Hygienists (ACGIH): None
  - National Toxicology Program (NTP): None
  - Occupational Safety and Health Administration (OSHA): None

- Chemical(s) subject to the reporting requirements of Section 313 or Title
  III of the Superfund Amendments and Reauthorization Act (SARA) of 1986 and
  40 CFR Part 372: Phosphoric acid

------------------------------------------------------------------------------
16. OTHER INFORMATION

US/Canadian Label Statements:

  CONTAINS: Stoddard Solvent (008052-41-3); Phosphoric acid (007664-38-2)

  WARNING!
  NOTICE! DELIBERATE CONCENTRATION AND INHALATION OF VAPORS MAY BE HARMFUL OR
  FATAL
  MAY BE HARMFUL IF SWALLOWED
  CAUSES SKIN AND EYE IRRITATION
  COMBUSTIBLE LIQUID AND VAPOR
  HIGH VAPOR CONCENTRATIONS MAY CAUSE DROWSINESS AND IRRITATION OF THE EYES OR
  RESPIRATORY TRACT
  CAN CAUSE CNS EFFECTS

  Keep away from heat and flame.
  Avoid prolonged or repeated breathing of mist or vapor.
  Avoid contact with eyes, skin, and clothing.
  Keep container closed.
  Use with adequate ventilation.
  Wash thoroughly after handling.

  FIRST AID: If swallowed, do NOT induce vomiting. Give victim a glass of
  water. Never give anything by mouth to an unconscious person. Call a
  physician or poison control center immediately. In case of contact,
  immediately flush eyes and skin with plenty of water for at least 15 minutes
  while removing contaminated clothing and shoes. Get medical attention. Wash
  contaminated clothing before reuse. Destroy or thoroughly clean contaminated
  shoes.

  IN CASE OF FIRE: Use water spray, carbon dioxide (CO2), dry chemical,
  alcohol foam. Use water spray to keep fire-exposed containers cool.

  IN CASE OF SPILL: Eliminate all ignition sources.

  Keep out of reach of children.

  For additional information, see Material Safety Data Sheet (MSDS) for this
  material.

  Since emptied containers retain product residue, follow label warnings even
  after container is emptied.
------------------------------------------------------------------------------
The information contained herein is furnished without warranty of any kind.
Users should consider these data only as a supplement to other information
gathered by them and must make independent determinations of suitability and
completeness of information from all sources to assure proper use and disposal
of these materials and the safety and health of employees and customers and
the protection of the environment.
------------------------------------------------------------------------------
R-1, S-2, F-2, C-0